**C900 Joint Restraint Available**

If you are having availability or rising price issues with your joint restraint for C900 pipe to pipe, we can help. The availability and pricing of internally and externally restrained C900 may be getting to be more of a challenge. Does your project call for bell joint harnesses, JM’s Eagle Loc, Diamond Pipe’s Diamond Loc, North American Pipe’s Certa Lok or Yelomine? You can now use standard C900 or IPS Class Pipe and either field install a RieberLok to replace a bell joint harness. Or you can buy RieberLok factory installed to replace the other factory installed type of restrained pipe. The RieberLok gasket is less expensive than both factory installed and bell joint harnesses, RieberLok is also much faster to install and is available now! The RieberLok is used in standard C900 pipe, which is much less expensive than the specialty pipe required for the other types. RieberLok is guaranteed to work and is available now in large quantities.

For use with all rieber type sockets 4"- 12" and 16" on C900 CIOD and 4"- 8" IPS

RieberLok is FM approved CIOD 4" thru 12"

ASTM D3139 compliant\*\*

For more information, Assembly Instructions, Field Cut Instruction, Casing Pull Instructions, and HDD Guidelines please go to:

[**www.RieberLok.com**](http://www.RieberLok.com)**.**

**McWane Global**

**Birmingham, AL**

**205-397-9464**